# Alerts

This view displays a list of faults, alarms, and events generated by the system, providing an oversight of issues that may require management or attention.

- Filter the alerts list by Type of alert, current State, and the Time period when the alert was generated.

- To filter alerts by floor, select Show alerts for selected plan and select the floor plan in the tree on the left.

- To remove the selected alert, click Clear.

- To acknowledge the selected alert, click Acknowledge. Enter any relevant details in the Comment dialog and click Ok to change the alert’s status to Acknowledged.

  | Only Fault and Alarm alerts can be acknowledged or cleared.

- Use the controls at the bottom of the screen to move to the Previous or Next page, and to adjust how many entries are displayed per page.

## Alert Information

Column | Description
--- | ---
Alert Icons | Created Fault Created Alarm Created Event Acknowledged Fault/Alarm Restored Cleared/Restore Acknowledged
Description | Description of the alert type
Source | Location of the alert
Date/Time | Date and time when the alert occurred
Type | Type of alert (Fault, Alarm, Event)
State | Created Acknowledged Cleared Restored Restore Acknowledged
Comments | Click the speech bubble icon to open the Details dialog.

#### Alert Comments and Details

The Details dialog shows the history of the selected alert, with controls to add a Comment and Acknowledge or Clear the alert.

## Alert Types

Alerts are classified by severity, into Faults (most severe), Alarms, and Events (least severe).

### Faults

- Device Offline

- Driver Offline

- Driver error

- Breaker Trip

- Functional Test

- Duration Test

- Sub Device Offline

- Custom Fault

### Alarms

- Logon Failure

- Panic

- Lamp Over Life

- Lamp Failure

- DyNet Over Voltage

- DyNet Under Voltage

- DyNet Voltage Interrupted

- Device Powered Down

- Green Power Down Failed

- Green Power Down Enable Failed

- Phase Failure

- Channel Electronic Fault Protection

- Channel Over Temperature

- FCUC Fire Trip

- FCUC Airflow Stopped

- FCUC Energy Holdoff

- FCUC Drip Tray Full

- FCUC Air Filter Dirty

- Temperature Sensor Open Circuit

- Temperature Sensor Short Circuit

- Temperature Sensor Remote Sensor Timeout

- Meter Value Over Reference

- Meter Value Under Reference

- Open Circuit Fault

- Short Circuit Fault

- Alarm DyNet Connection Offline

- Alarm FIAS Connection Offline

- Deployment (Room Configuration)

- Deployment (Room Variables)

- Meter Value Out of Range

- Custom Alarm

### Room Alarms (Interact Multiroom)

- Balcony Door Open

- Devices Offline

- Do Not Disturb

- Entrance Dorr Open

- FCUC Air Filter Dirty

- FCUC Drip Tray Full

- Guest Well-being

- Humidity

- Laundry Pickup

- Make Up Room

- Room Safe Closed at Check-out

- Room Service Response

- Room Temperature

- Soil Moisture

- Water Leak

### Events

- User Log On

- User Log Off

- Schedule Started

- Schedule Stopped

- Schedule Enabled

- Schedule Disabled

- Trigger Enabled

- Trigger Disabled

- Report Ran

- Database Backup

- Database Purge

- Public Holidays Update

- Macro Started

- Macro Stopped

- Macro Paused

- Macro Resumed

- All Macros Stopped

- Emergency Group Function Test Started

- Emergency Driver Function Test Started

- Emergency Group Duration Test Started

- Emergency Driver Duration Test Started

- Emergency Group Function Test Stopped

- Emergency Driver Function Test Stopped

- Emergency Group Duration Test Stopped

- Emergency Driver Duration Test Stopped

- Emergency Group Function Test Completed

- Emergency Driver Function Test Completed

- Emergency Group Duration Test Completed

- Emergency Driver Duration Test Completed

- Lamp End of Life

- Sensor Calibration Complete

- Panels Enabled

- Panels Disabled

- Motion Control Enabled

- Motion Control Disabled

- PE Control Enabled

- PE Control Disabled

- Area Cascading Enabled

- Area Cascading Disabled

- Custom Event

- Channel Level Sent

- Channel Temperature Sent

- Console button clicked (by SM user)

- Preset Sent (by SM user)

- Save Preset sent (by SM user)