# OPC UA Objects

OPC UA stores configuration data in objects. The table below shows the configuration data that SM can map to OPC UA objects.

Object properties | Data Points | Methods | Alarms
--- | --- | --- | ---
Areas Data Point Area Name Area No | Current Preset No Current Temperature Metered Power Motion Timeout Notional Power Setpoint Temperature Total Offline Devices Total Offline Drivers or Lamps | SetAreaPreset SetAreaTemperature SetAreaTemperatureUpDown |
DALI Devices Data Point Device Code Device Index Device Name Product Name | Online Status |  | DeviceStatusAlarm
DALI Sensors Data Point Device Code Device Index Device Location Device Name Product Name | LUX Level |  |
Devices Data Point Box Number Device Code Device Name Product Name | Online Status |  | DeviceStatusAlarm
Emergency Test Groups [Group Name] Data Point Emergency Group ID | Total Duration Test Failure Total Duration Test Running Total Duration Test Success Total Functional Test Failure Total Functional Test Running Total Functional Test Success Total Emergency Drivers |  |
General System Health Data Point | DyNet Connection Status Total Offline Devices Total Offline Drivers Total Offline Lamps Total Offline Trunk Gateways Total Trunk Gateways |  | DyNetConnectionOfflineAlarm
Load Control Channels Data Point Box Number Channel Name Channel No Device Code Device UID Product Name | Channel Runtime Driver Status Lamp Status |  | DriverOfflineAlarm LampOfflineAlarm
Logical Channels Data Point Area No Channel Name Channel No | Channel Level | SetLogicalChannelLevel |
Sensors Data Point Box Number Device Code Device Location Device Name Product Name | LUX Level |  |