# SM Switch Installation

The System Manager installer offers Switch as an optional application during installation.
Switch is a client of the SM server and settings are loaded from the SM server database.

Install Switch:

1. Copy the `C:\Philips Dynalite\System Manager\Switch` folder from the SM server to the same location on the client PC.

2. On the client PC, open File Explorer and navigate to `C:\Philips Dynalite\System Manager\Switch`.

3. Right-click `Setup.exe` and select Run as administrator.

4. When installation is complete, click Done to close the installer.

Once installed and launched, Switch runs in the background. You can launch Switch from the Start menu, or add it to the Windows Startup Apps list to launch it automatically. Switch can be installed on any number of PCs connected to the same LAN as the Dynalite system.

## Shared client upgrades

You can distribute new versions of Switch via a shared folder along with SM client upgrades.
See Automatic Client Upgrades for more information.